Custom Feature

# Deck Railing
Installation

Install code-compliant deck railings that protect your family and define your outdoor space. We work with aluminum balusters, cable systems, glass panels, and composite materials—matched to your deck's style and your budget.

Get Free Estimate
Call (612) 655-8664

## Railings Built to Code, Designed to Last

Deck railings serve two purposes: safety and style. Minnesota building code mandates railings on any deck surface 30 inches or more above grade, with specific requirements for height, baluster spacing, and structural load capacity. We install railings that meet or exceed all code requirements while matching your deck's aesthetic.

Our railing systems use powder-coated aluminum balusters, composite or PVC post sleeves, and stainless steel fasteners rated for exterior use. Every component resists Minnesota's freeze-thaw cycles, UV exposure, and moisture—no annual painting or staining required.

- 36" or 42" heights (code-compliant)
- Aluminum, composite, and PVC materials
- Cable, glass, and traditional baluster infills
- Powder-coated finishes in 20+ colors
- Retrofit installation on existing decks

Request Railing Consultation
Railing Options

## Types of Deck Railings We Install

Choose from several railing systems based on your view preferences, maintenance tolerance, and budget. We help you select the right combination of posts, rails, and infill materials.

### Aluminum Balusters

Powder-coated aluminum balusters paired with composite or wood rails. Available in round, square, and decorative profiles. Zero maintenance and 25-year warranties typical.

### Cable Railing

Horizontal stainless steel cables with aluminum or wood posts. Maximizes sightlines and creates a modern aesthetic. Requires periodic tensioning to maintain proper cable tautness.

### Glass Panel Railings

Tempered safety glass panels for unobstructed views. Ideal for lakefront or scenic properties. Available in clear, tinted, or frosted options. Wind-resistant and code-compliant.

### Wood & Metal Hybrid

Cedar or pressure-treated wood posts and rails with aluminum baluster infills. Traditional appearance with reduced maintenance. Requires periodic staining or sealing of wood components.

### Composite Systems

All-composite posts, rails, and sometimes balusters. Color-matched to composite decking brands like Trex, TimberTech, and Fiberon. Consistent appearance with zero wood maintenance.

### Elevated Deck Railings

Engineered for second-story and walkout basement decks. 42" height required for decks over 30" above grade. Reinforced post mounting to meet structural load requirements.

Building Code

## Minnesota Deck Railing Requirements

All deck railings we install meet Minnesota Residential Code requirements. Here's what the code specifies:

Railing Height

Minimum 36" for decks up to 30" above grade. Minimum 42" for decks more than 30" above grade. Measured from deck surface to top of rail.

Baluster Spacing

Maximum 4" between balusters (a 4" sphere cannot pass through). This prevents children from getting stuck or falling through openings.

Load Capacity

Rails must withstand 200 lbs concentrated load or 50 lbs/ft distributed load. Posts must resist lateral loads without deflection exceeding code limits.

Graspable Handrail

Stairs require a graspable handrail (1.25" to 2" diameter) continuous along the full stair length, extending beyond top and bottom risers.

Our Work

## Railing Installation Projects

Browse completed railing installations across Elk River and surrounding Minnesota communities.

Related Services

## Complete Your Deck Project

Deck railings pair with these services. Bundle features during new construction or upgrades for best value.

### Deck Lighting

Add LED post cap lights to your railing posts. Pre-wire during railing installation for clean wiring runs through post interiors.

View lighting options

### Custom Deck Building

Build a new deck with integrated railing posts. Proper post-to-frame connections are strongest when built together.

Learn more

### Deck Repair & Restoration

Replace worn railings during deck repairs. We inspect post connections and rim joist integrity before new railing installation.

Learn more

## Ready for New
Deck Railings?

Schedule a free consultation to discuss railing options for your deck. We'll measure your space, review material choices, and provide a detailed estimate.

Schedule Free Consultation